Atlas Copco

No

Crawler Drill

Drfter

Part Number

Part Name

Q'ty

Unit Price

Remarks

3115 1605 90

set of nipple

1set

COP1440

\*}

front head

COP1440

3115 0286 00

dome nut

0.26kg

COP1440

3115 0287 00

washer

0.04kg

COP1440

0147 1401 03

screw

COP1440

3115 1938 00

connection plate

1.54kg

COP1440

0665 1000 12

cup seal

COP1440

3176 6518 00

nipple, 25mm

0.26kg

COP1440

3115 1457 00

side bolt

0.82kg

COP1440

cover, compl.

5kg

COP1440

\*}

.cover

COP1440

0666 7190 01

.seal ring

0.06kg

COP1440

0335 3576 00

.lock ring

0.02

COP1440

0102 0473 00

cylindrical pin

COP1440

0663 6151 00 \*\*}

o-ring

COP1440

3115 0297 01

shim, 0.10mm

0.1

COP1440

3115 0297 02

shim, 0.15mm

0.15

COP1440

3115 0297 03

shim, 0.3mm

0.5

COP1440

0509 0223 00

roller bearing 32018XQ

1.8kg

COP1440

3115 0285 00

side bolt

3115 2113 00

3115 5040 00

COP1440

shank adapter

COP1440

3115 1582 00

driver

1.66kg

COP1440

3115 1732 81

rotation chuck, compl.

4.44kg

COP1440

\*}

.rotation chuck

COP1440

3115 1881 00

.bushing

0.18kg

COP1440

0509 0221 00

roller bearing 32016XQ

1.3kg

COP1440

3115 1365 80

gear housing, compl.

1

COP1440

\*}

.gear housing

COP1440

0686 6101 00

.plug

COP1440

0644 2162 00

.lubricating nipple

COP1440

0666 7188 01

.seal ring

0.04

COP1440

0335 3572 00

.lock ring

0.01

COP1440

3115 0273 00

.washer

0.02

COP1440

0663 2120 00 \*\*}

o-ring

COP1440

0663 6146 00 \*\*}

o-ring

COP1440

3115 2064 00

rotation chuck bushing

1.38kg

COP1440

3115 0821 80

shaft, compl.

2.1kg

27,29,30,31,26,32 set

COP1440

\*}

.shaft

COP1440

0516 1504 01

.needle bearing

0.06kg

COP1440

3115 0823 00

.washer

0.02kg

COP1440

0516 1638 00

.needle bearing

COP 1440 Drifter Parts for Atlas Copco

COP1440

3115 0824 00

.sleeve

0.2kg

COP1440

0667 1206 00

.cup seal

0

COP1440

3115 0625 00

.guide sleeve

COP1440

38

COP1440

3115 0274 00

gear

0.64kg

39

COP1440

0663 2133 01

o-ring

40

COP1440

3115 1846 00

damping piston

41

COP1440

B}

set of seals

42

COP1440

3115 2083 00

liner

43

COP1440

0663 6144 00

o-ring

44

COP1440

0663 6142 00

o-ring

45

COP1440

0335 3500 10

lock ring

46

COP1440

3115 2084 00

bushing

0.08kg

47

COP1440

B}

set of seals

COP1440

3115 2071 80

intermediate part, compl.

48

COP1440

\*}

.intermediate part

COP1440

0259 2061 00

.thread insert

COP1440

0259 0068 00

.thread insert

49

COP1440

3115 1746 06

.nozzle

50

COP1440

3115 1458 00

connection plate

3115 3455 00

51

COP1440

0211 1402 00

screw

52

COP1440

0663 2100 62 \*\*}

o-ring

53

COP1440

3115 1763 82

high pressure accumulator

54

COP1440

3115 1854 80

compl.

55

COP1440

0147 1483 03

low pressure accumulator compl

COP1440

3115 1103 80

seal housing, compl.

0.40kg

56

COP1440

\*}

.seal housing

57

COP1440

3115 0970 00

.set of seals

58

COP1440

0663 6136 00 \*\*}

.o-ring

59

COP1440

0663 6142 00 \*\*}

o-ring

60

COP1440

3115 1671 00

piston guide, front

3115 5050 01

0.28KG

61

COP1440

0663 6134 01 \*\*}

o-ring

62

COP1440

3115 1765 00

valve piston

0.38kg

63

COP1440

3115 1831 00

valve cover, left

64

COP1440

3115 1830 00

valve cover, right

65

COP1440

F

screw

66

COP1440

0147 1487 03

screw

67

COP1440

3115 1697 00

seal washer

68

COP1440

3115 1692 00

dome nut

0.06

69

COP1440

3115 1530 00

regulating plug

COP1440

COP1440

3115 1767 80

cylinder, compl.

71

COP1440

\*}

.cylinder

72

COP1440

3115 1825 00

..pipe plug

73

COP1440

0661 1034 00

..seal washer

COP1440

0259 0011 00

..thread insert

COP1440

0259 0311 00

..thread insert

74

COP1440

0686 6447 04

..plug

75

COP1440

3115 0276 00

.guide

0.16

76

COP1440

3115 1166 00

.stud

77

COP1440

3115 0277 00

coupling

0.38kg

78

COP1440

0335 2130 00

circlip

79

COP1440

3115 1010 80,81

hydraulic motor

10.5kg

80

COP1440

3115 1454 00

nut

81

COP1440

0663 2115 00 \*\*}

o-ring

82

COP1440

3115 1970 00

piston

3115 2838 00

6kg

83

COP1440

0663 6137 00 \*\*}

o-ring

84

COP1440

3115 1833 00

piston guide, rear

0.34

COP1440

3115 1832 80

seal housing, compl.

85

COP1440

\*}

.seal housing

86

COP1440

3115 0845 00

.set of seals

87

COP1440

0663 6135 00 \*\*}

.o-ring

88

COP1440

3115 1829 00

back head

89

COP1440

0291 1180 02

lock nut

90

COP1440

3176 6512 00

nipple

91

COP1440

3176 5313 00

cap

92

COP1440

3176 6514 00

nipple (1/2", draining)

93

COP1440

3715 0597 00

cap

COP1440

optional equipment

COP1440

3115 9150 92

o-ring set

COP1440

\*\*\*}

special tools set

COP1440

3115 0978 00

pressure gauge

COP1440

0371 1102 00

lifting eye

47

COP1440

3115 2074 90

set of seals

COP1440

COP1440

3115 1983 80

front head, compl.

1

COP1440

\*}

.front head

2

COP1440

3115 2223 00

.guide

3

COP1440

0663 2103 58 \*\*}

.o-ring

4

COP1440

3115 2055 00

.set of seals

5

COP1440

3115 2225 00

.bushing

6

COP1440

0335 3500 12

.lock ring

7

COP1440

0663 2101 66 \*\*}

.o-ring

8

COP1440

3115 2116 00

.set of seals

9

COP1440

3115 2634 00

.bushing

10

COP1440

3115 2520 00

piston

11

COP1440

3115 0286 00

dome nut

0.26kg

12

COP1440

3115 0287 00

washer

0.04kg

13

COP1440

3115 2221 00

stud

14

COP1440

3176 6514 00

nipple (intake)

15

COP1440

3715 0597 00

cap

16

COP1440

3176 6512 00

nipple (return)

17

COP1440

3176 5313 00

cap

19

COP1440

3176 6566 00

nipple

20

COP1440

3176 6509 00

nipple

21

COP1440

3176 6618 00

nut

22

COP1440

0102 0460 00

cylindrical pin

COP1440

3115 2314 80

cover, compl.

23

COP1440

\*}

.cover

24

COP1440

0666 7190 01

.radial lip seal

0.06kg

25

COP1440

0335 2173 00

.circlip

0.04

26

COP1440

0663 6143 01 \*\*}

o-ring

27

COP1440

3115 2387 00

cup seal

28

COP1440

3115 2315 00

flushing head

29

COP1440

3115 2222 00

side bolt

31

COP1440

7304 3825 02

shank adapter, T38E

31

COP1440

7305 3826 02

shank adapter, T45E

31

COP1440

7306 3828 02

shank adapter, T51E

32

COP1440

3115 2317 00

flushing connection

33

COP1440

0661 2014 00

back up ring

34

COP1440

0663 9166 01 \*\*}

o-ring

35

COP1440

0663 2126 01 \*\*}

o-ring

36

COP1440

0196 1318 00

set screw

COP1440

optional equipment

37

COP1440

3115 2231 00

drill collar (for drilling upwards T38)

37

COP1440

3115 2232 00

drill collar (for drilling upwards T45)

37

COP1440

3115 2233 00

drill collar (for drilling upwards T51)

COP1440

1

COP1440

3115 1945 00

front head

2

COP1440

3115 1938 00

connection plate

1.54kg

3

COP1440

0665 1000 12

cup seal

4

COP1440

3315 0195 08

lock washer

5

COP1440

0147 1401 03

screw

6

COP1440

3176 6518 00

nipple

0.26kg

7

COP1440

3115 2118 00

guide

1.9kg

8

COP1440

3115 2333 00

cup seal

3115 3364 00

0.04kg

9

COP1440

0663 2145 01 \*\*}

o-ring

10

COP1440

3115 2120 00

flushing head

4.3kg

11

COP1440

0665 0999 21

cup seal

3115 5190 00

12

COP1440

3115 2122 00

stop ring

1.58KG

13

COP1440

0663 2143 00 \*\*}

o-ring

14

COP1440

3115 2119 00

guide

1.36kg

15

COP1440

3115 2386 00

cup seal

16

COP1440

3115 2121 00

flushing head

4.5kg

17

COP1440

3115 2693 00

cup seal

COP1440

3115 2117 60

stop ring, compl.

COP1440

3115 2123 80

stop ring, compl.

1.6kg

18

COP1440

\*}

.stop ring (split)

19

COP1440

0663 2105 96 \*\*}

.o-ring

20

COP1440

7304 3652 01

shank adapter, T38

21

COP1440

7603 3655 01

shank adapter, R32E

21

COP1440

7604 3655 01

shank adapter, T38E

21

COP1440

7305 3655 01

shank adapter, T45E

21

COP1440

7306 3655 01

shank adapter, T51E

21

COP1440

7603 3656 01

shank adapter, R32E

21

COP1440

7604 3652 01

shank adapter, R38

21

COP1440

7304 3656 01

shank adapter, T38E

COP1440

optional equipment

22

COP1440

3115 2231 00

drill collar (for drrilling upwards R32/T38)

22

COP1440

3115 2232 00

drill collar (for drrilling upwards T45)

22

COP1440

3115 2233 00

drill collar (for drrilling upwards T51)

COP1440

COP1440

3115 1854 80

low pressure accumulator

1

COP1440

3115 1876 00

housing

2

COP1440

3115 1822 00

diaphragm

0.04kg

3

COP1440

3115 1854 00

cover

COP1440

3115 0262 00

valve, compl.

0.04kg

4

COP1440

\*}

.valve

5

COP1440

3310 4076 00

.cap

6

COP1440

0663 9056 00 \*\*}

o-ring

COP1440

COP1440

3115 1010 93

set of seals

1

COP1440

3115 1010 47

bearing housing

2

COP1440

\*\*}

seal ring

3

COP1440

3115 1010 48

splined shaft

4

COP1440

\*\*}

seal ring

5

COP1440

\*\*}

o-ring

6

COP1440

3115 1010 42

intermediats parts

7

COP1440

3115 1010 27

drain plug

8

COP1440

3115 1010 58

washer

9

COP1440

3115 1010 07

cardan shaft

9

COP1440

3115 1010 29

cardan shaft

10

COP1440

\*\*}

o-ring

11

COP1440

3115 1010 43

cog wheel set

11

COP1440

3115 1010 50

cog wheel set

12

COP1440

3115 1010 10

guide pin

13

COP1440

3115 1010 12

valve drive

14

COP1440

3115 1010 13

channel plate

15

COP1440

3115 1010 14

disc valve

16

COP1440

3115 1010 15

balance plate

17

COP1440

3115 1010 16

guide pin

18

COP1440

\*\*}

o-ring

19

COP1440

\*\*}

o-ring

20

COP1440

3115 1010 19

spacer pin

21

COP1440

3115 1010 20

spring ring

22

COP1440

3115 1010 21

valve housing

23

COP1440

\*\*}

seat plug

24

COP1440

3115 1010 44

screw

24

COP1440

3115 1010 52

screw

25

COP1440

\*\*}

seal ring

26

COP1440

3115 1010 23

check valve ball

27

COP1440

3115 1010 62

check valve spring

28

COP1440

3115 1010 63

check valve plug

29

COP1440

3115 1010 64

washer

COP1440

COP1440

3115 1763 82[

구형

]

3115 2696 80[

신형

]

3115 3511 81

4.04KG

1

COP1440

3115 1876 00

housing

2

COP1440

3115 1822 00

diaphragm

0.04kg

3

COP1440

3115 0263 00

plug

4

COP1440

0653 6121 00 \*\*}

o-ring

5

COP1440

3115 1763 00

cover

COP1440

3115 062 00

valve, compl.

6

COP1440

\*}

.valve

7

COP1440

3310 4076 00

.cap

COP1440

0147 1483 03

screw

8

COP1440

0663 9056 00 \*\*}

o-ring

COP1440

COP1440

front head

1

COP1440

3115 1362 00

front head

10.20kg

2

COP1440

3115 1436 00

guide

1.1kg

3

COP1440

0667 3194 00

cup seal

4

COP1440

0663 2145 01 \*\*}

o-ring

5

COP1440

3115 2078 00

flushing head

4.2kg

6

COP1440

3115 1434 00

stop ring

1.4kg

17

COP1440

7804 3652 01

shank adapter R38 (17.1 in)

17

COP1440

7803 3656 01

shank adapter R32 (20.7 in)

17

COP1440

7304 3652 01

shank adapter T38 (17.1 in)

17

COP1440

7304 3656 01

shank adapter T38 (20.7 in)

COP1440

COP1440

set of nipples

COP1440

3115 1603 90

set of nipples, compl.

1.04kg

COP1440

3177 3046 00

.nipple for impact mechanism, intake

COP1440

3176 6567 00

.nipple for impact mechanism, intake

COP1440

3176 6565 00

.nipple for rotation motor, intake/return

COP1440

3115 1459 00

.nipple for rotation motor, intake/return

COP1440

3176 6515 00

.nipple for rotation motor, intake/return

COP1440

3176 6349 00

.nipple for lub.air.hose 1/4" for oil-fog lubricator DIM